(kicad_symbol_lib (version 20210619) (generator kicad_symbol_editor)
  (symbol "comm:NEO-8Q" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 0 13.97 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "NEO-8Q" (id 1) (at 0 -27.94 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 0 0 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "NEO-8Q_0_1"
      (rectangle (start -12.7 11.43) (end 13.97 -24.13)
        (stroke (width 0.1524)) (fill (type background))
      )
    )
    (symbol "NEO-8Q_1_1"
      (pin input line (at 16.51 -21.59 180) (length 2.54)
        (name "SAFEBOOT_N" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 3.81 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "10" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 6.35 180) (length 2.54)
        (name "RF_IN" (effects (font (size 1.27 1.27))))
        (number "11" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 8.89 180) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "12" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 8.89 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "13" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -15.24 6.35 0) (length 2.54)
        (name "LNA_EN" (effects (font (size 1.27 1.27))))
        (number "14" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at -15.24 3.81 0) (length 2.54)
        (name "Reserved" (effects (font (size 1.27 1.27))))
        (number "15" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at -15.24 1.27 0) (length 2.54)
        (name "Reserved" (effects (font (size 1.27 1.27))))
        (number "16" (effects (font (size 1.27 1.27))))
      )
      (pin free line (at -15.24 -1.27 0) (length 2.54)
        (name "Reserved" (effects (font (size 1.27 1.27))))
        (number "17" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -6.35 0) (length 2.54)
        (name "SDA/SPICS_N" (effects (font (size 1.27 1.27))))
        (number "18" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at -15.24 -8.89 0) (length 2.54)
        (name "SCL/SPICLK" (effects (font (size 1.27 1.27))))
        (number "19" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -19.05 180) (length 2.54)
        (name "D_SEL" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -15.24 -11.43 0) (length 2.54)
        (name "TDX/SPIMISO" (effects (font (size 1.27 1.27))))
        (number "20" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -13.97 0) (length 2.54)
        (name "RDX/SPIMOSI" (effects (font (size 1.27 1.27))))
        (number "21" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -16.51 0) (length 2.54)
        (name "V_BCKP" (effects (font (size 1.27 1.27))))
        (number "22" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -19.05 0) (length 2.54)
        (name "VCC" (effects (font (size 1.27 1.27))))
        (number "23" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -15.24 -21.59 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "24" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 -16.51 180) (length 2.54)
        (name "TIMEPULSE" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -13.97 180) (length 2.54)
        (name "EXTINT" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -11.43 180) (length 2.54)
        (name "USB_DM" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin bidirectional line (at 16.51 -8.89 180) (length 2.54)
        (name "USB_DP" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -6.35 180) (length 2.54)
        (name "VDD_USB" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 16.51 -1.27 180) (length 2.54)
        (name "RESET_N" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 16.51 1.27 180) (length 2.54)
        (name "VCC_RF" (effects (font (size 1.27 1.27))))
        (number "9" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "comm:TPS2116" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TPS2116" (id 1) (at 3.81 -8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TPS2116_0_1"
      (rectangle (start -2.54 11.43) (end 10.16 -6.35)
        (stroke (width 0.1524)) (fill (type background))
      )
    )
    (symbol "TPS2116_1_1"
      (pin input line (at -5.08 7.62 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.08 3.81 0) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 0 0) (length 2.54)
        (name "VIN1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -3.81 0) (length 2.54)
        (name "PR1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 7.62 180) (length 2.54)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 3.81 180) (length 2.54)
        (name "VIN2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -3.81 180) (length 2.54)
        (name "ST" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
  (symbol "comm:TSP2116" (in_bom yes) (on_board yes)
    (property "Reference" "U" (id 0) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "TSP2116" (id 1) (at 3.81 -8.89 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "" (id 2) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "" (id 3) (at 3.81 12.7 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (symbol "TSP2116_0_1"
      (rectangle (start -2.54 11.43) (end 10.16 -6.35)
        (stroke (width 0.1524)) (fill (type background))
      )
    )
    (symbol "TSP2116_1_1"
      (pin input line (at -5.08 7.62 0) (length 2.54)
        (name "GND" (effects (font (size 1.27 1.27))))
        (number "1" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at -5.08 3.81 0) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "2" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 0 0) (length 2.54)
        (name "VIN1" (effects (font (size 1.27 1.27))))
        (number "3" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at -5.08 -3.81 0) (length 2.54)
        (name "PR1" (effects (font (size 1.27 1.27))))
        (number "4" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 7.62 180) (length 2.54)
        (name "MODE" (effects (font (size 1.27 1.27))))
        (number "5" (effects (font (size 1.27 1.27))))
      )
      (pin input line (at 12.7 3.81 180) (length 2.54)
        (name "VIN2" (effects (font (size 1.27 1.27))))
        (number "6" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 0 180) (length 2.54)
        (name "VOUT" (effects (font (size 1.27 1.27))))
        (number "7" (effects (font (size 1.27 1.27))))
      )
      (pin output line (at 12.7 -3.81 180) (length 2.54)
        (name "ST" (effects (font (size 1.27 1.27))))
        (number "8" (effects (font (size 1.27 1.27))))
      )
    )
  )
)
