
(kicad_symbol_lib (version 20211014) (generator kicad_symbol_editor)
  (symbol "USB4110-GF-A_REVB" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
    (property "Reference" "J" (id 0) (at -12.7 11.43 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Value" "USB4110-GF-A_REVB" (id 1) (at -12.7 -15.24 0)
      (effects (font (size 1.27 1.27)) (justify bottom left))
    )
    (property "Footprint" "GCT_USB4110-GF-A_REVB" (id 2) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "PARTREV" "B" (id 4) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MAXIMUM_PACKAGE_HEIGHT" "3.26 mm" (id 5) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "STANDARD" "Manufacturer Recommendations" (id 6) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (property "MANUFACTURER" "GCT" (id 7) (at 0 0 0)
      (effects (font (size 1.27 1.27)) (justify bottom) hide)
    )
    (symbol "USB4110-GF-A_REVB_0_0"
      (rectangle (start -12.7 -12.7) (end 12.7 10.16)
        (stroke (width 0.254)) (fill (type background))
      )
      (pin bidirectional line (at -17.78 2.54 0) (length 5.08)
        (name "CC1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 0.0 0) (length 5.08)
        (name "DP1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -2.54 0) (length 5.08)
        (name "DN1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at -17.78 -5.08 0) (length 5.08)
        (name "SBU1"
          (effects (font (size 1.016 1.016)))
        )
        (number "A8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 7.62 180.0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "A4/B9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 7.62 180.0) (length 5.08)
        (name "VBUS"
          (effects (font (size 1.016 1.016)))
        )
        (number "B4/A9"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 2.54 180.0) (length 5.08)
        (name "CC2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B5"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 0.0 180.0) (length 5.08)
        (name "DP2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B6"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -2.54 180.0) (length 5.08)
        (name "DN2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B7"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin bidirectional line (at 17.78 -5.08 180.0) (length 5.08)
        (name "SBU2"
          (effects (font (size 1.016 1.016)))
        )
        (number "B8"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "A1/B12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "B1/A12"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "S1"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "S2"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "S3"
          (effects (font (size 1.016 1.016)))
        )
      )
      (pin power_in line (at 17.78 -10.16 180.0) (length 5.08)
        (name "GND"
          (effects (font (size 1.016 1.016)))
        )
        (number "S4"
          (effects (font (size 1.016 1.016)))
        )
      )
    )
  )
)